{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求 ","技术参数"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求 ","index":0,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,4],[0,8,1,10],[2,10,2,11],[2,12,2,13],[5,0,5,4],[6,0,6,4]],"flags":["formulas_cached_only"]}
["采购项目清单： 妇女儿童医院太平间太平柜采购"]
[]
["序号","项目名称","规格","拦标价（元）","备注"]
["1、","六门分体组装式太平柜",null,58000]
[]
[]
["技术要求及配置确认书\n一、项目名称、数量：妇女儿童医院太平间太平柜采购 \n二、项目用途说明：我院妇女儿童医院已经开诊，太平间内需安装太平柜用于冷冻死婴、死胎、遗体等，经医院决定进行公开招标。                             \n三、配置规格、附件及零配件（包括专用工具）：1、提供由第三方出具的检测报告（主要是太平柜温度控制）。2、清单及技术参数要求见附件。                                                     \n四、详细技术要求、参数及产品资料等：①、税务登记证、营业执照、组织机构代码或三证合一的营业执照；②、法人签字并加盖公章的委托书；③、投标人的身份证及复印件；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；⑤、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。 \n                                                         \n五、售后服务条件及交货日期（或工期）：质量承诺（包括质保期及质保金）   \n                                                             \n                                                        \n五、推荐供应商清单\n    一、除公开招标、单一来源外的其他院内采购方式，可推荐三家以上供应商，并且要具有可比性。\n    二、填写内容包括供应商名称、联系人、联系方式，产地、品牌或资质。\n推荐供应商1                                                \n                                                         \n推荐供应商2                                                \n                                                         \n推荐供应商3                                                \n                                                         \n推荐供应商4                                                \n                                                         \n推荐供应商5                                             "]

{"sheet":"技术参数","index":1,"n_rows":19,"n_cols":3,"rows_kept":19,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
[" 采购需求及要求"]
["序号","项目","产品技术规格、参数"]
[1,"结构","组合式，可折叠，单门单控，现场安装机组"]
[2,"规格","外部：长 2.2 X宽0.8X高1.9（米）内部≥2.0x0.6x0.5(米）±10%的偏差"]
[3,"外墙材质","采用304不锈钢  厚度≥l.0mm"]
[4,"内胆材质","内胆为≥0.6mm304不锈钢，内胆底部凹槽式。"]
[5,"柜门","304不锈钢（厚≥1.0mm）凸装门，带加热除露功能。"]
[6,"托板","框架采用优质不锈钢方管（≥25X25mm）、内铺设304不锈钢板（≥0.8mm）"]
[7,"助力导轮","不锈钢轮≥Ф12x30（mm）不锈钢滑道"]
[8,"蒸发器","直冷内置式盘管蒸发器，铜管直径为≥10mm,厚度为≥0.6mm，长为≥40m铜管分别铺设于内箱体的顶部和两侧"]
[9,"冷凝器","采用风冷翅片式盘管冷凝器，面积（≥4.0m²）"]
[10,"保温材料","采用聚氨酯发泡材料，（每立方密度为≥40.6），厚度为≥100mm"]
[11,"机组形式","高性能优质压缩机（3台），对冷藏柜各层分别控制"]
[12,"额定制冷温度","空间温度 -10℃-18℃"]
[13,"制冷剂","环保型R290"]
[14,"功率","≥1500w"]
[15,"电源","≥220V"]
[16,"温度控制","微电脑全自动温度控制器"]
[" "]