{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","技术参数"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,4],[0,7,1,8],[2,8,2,9],[2,10,2,11],[5,0,5,1],[5,2,5,4],[6,0,6,4]],"flags":["formulas_cached_only"]}
["采购项目清单：妇女儿童医院污水站第三方检测服务采购"]
[]
["序号","项目名称","数量或规模","资金预算","资金来源"]
["1、","妇女儿童医院污水站第三方检测服务采购","一年","6万元","自筹"]
["合计"]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：妇女儿童医院污水站第三方检测服务采购\n二、项目用途说明：妇女儿童医院污水站排污许可证已办理，按照环保要求医院污水处理水质和废气等排放指标应经第三方检测公司进行检测并出具检测报告，现决定对该项目进行院内竞争性谈判采购                           \n三、配置规格、附件及零配件（包括专用工具）： 投标人应具备的资格条件：1、具有独立承担民事责任的能力；2、具有良好的商业信誉和健全的财务会计制度；3、具有履行合同所必需的设备和专业技术能力；4、有依法缴纳税收和社会保障资金的良好记录；5、参加政府采购活动前三年内，在经营活动中没有重大违法记录；6、响应供应商应依法取得相关资质，提供检验检测机构资质认定证书；7、不接受联合体投标。8、提供近三年以来具有医院类似服务业绩的同等条件下优先（提供业绩合同原件，并附合同对应的复印件）。9、具体检测项目见附件。                                                        \n四、详细技术要求、参数及产品资料等：                                                                                                                                                                                 ①、税务登记证、营业执照、组织机构代码或三证合一的营业执照；②、法人签字并加盖公章的委托书；③、投标人的身份证及复印件；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。                                                      \n五、售后服务条件及交货日期（或工期）：质量承诺（包括质保期及质保金）\n                         五、推荐供应商清单\n一、除公开招标、单一来源外的其他院内采购方式，可推荐三家以上供应商，并且要具有可比性。\n二、填写内容包括供应商名称、联系人、联系方式，产地、品牌或资质。\n推荐供应商1                                                \n                                                         \n推荐供应商2                                                \n                                                         \n推荐供应商3                                                \n                                                         \n推荐供应商4                                                \n                                                         \n推荐供应商5                                             "]

{"sheet":"技术参数","index":1,"n_rows":33,"n_cols":4,"rows_kept":33,"merged":[[0,0,0,3],[2,0,4,0],[5,0,7,0],[8,0,10,0],[11,0,13,0],[14,0,18,0],[19,0,31,0]],"flags":["formulas_cached_only"]}
["妇女儿童医院污水站第三方检测项目清单"]
["分类","检测项目","频次，次/天","次/年度"]
["锅炉废气排放口1","二氧化硫",3,1]
[null,"氮氧化物",3,1]
[null,"颗粒物",3,1]
["锅炉废气排放口2","二氧化硫",3,1]
[null,"氮氧化物",3,1]
[null,"颗粒物",3,1]
["锅炉废气排放口3","二氧化硫",3,1]
[null,"氮氧化物",3,1]
[null,"颗粒物",3,1]
["污水处理废气排放口DA001","臭气浓度",3,4]
[null,"氨",3,4]
[null,"硫化氢",3,4]
["污水处理站周界","氯",16,4]
[null,"甲烷",16,4]
[null,"臭气浓度",16,4]
[null,"氨",16,4]
[null,"硫化氢",16,4]
["污水处理站排放口DW001","阴离子表面活性剂",3,4]
[null,"动植物油",3,4]
[null,"总余氯",3,4]
[null,"总氰化物",3,4]
[null,"挥发酚",3,4]
[null,"氨氮（NH3-N）",3,4]
[null,"色度",3,4]
[null,"石油类",3,4]
[null,"五日生化需氧量",3,4]
[null,"化学需氧量",3,4]
[null,"悬浮物",3,52]
[null,"pH值",3,52]
[null,"粪大肠菌群",3,12]
["接触池出口","总余氯",3,52]